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The remodelled Melangeursplein square in the Dutch city of Zevenaar combines historical industrial architecture with open, green recreational spaces.
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The Mono-Fortis heavy-duty channel produced by Richard Brink facilitates linear dewatering along the paved sections of the square.

Photo: Richard Brink GmbH & Co. KG



	

[image: ]




	

RichardBrink_Zevenaar_03


	

The monolithic channel elements made from polymer concrete blend seamlessly into the paving to create a clear, continuous line.
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The channel bodies and gratings in the Mono-Fortis range are comprised of a single polymer-concrete component. Despite its comparatively light weight, the channel is extremely resilient, meeting the requirements of load class E 600.
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A total of four drainage units with matching Zippa designer cast gratings complete the 66-metre-long dewatering line.
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In combination, the polymer-concrete channels and drainage units impress with their high load capacity while still blending discreetly into the public space.
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